
English:

/---------------------\
|                     |
| New Bootloader V2.1 |
|                     |
\---------------------/

For roloFlash with a firmware older than v07.** a one-time update of
the bootloader is needed. This is required to update to newer firmware
versions. With the new bootloader, you can still downgrade roloFlash
to older firmware versions.

Please precisely follow description for the bootloader update in the
manual, chapter "Updating the bootloader". The files RF2A06ZZ.HMP and
RF2_06ZZ.HMP are used for this update.


--------------------------------------------------------------------------------

Deutsch:

/-----------------------\
|                       |
| Neuer Bootloader V2.1 |
|                       |
\-----------------------/

Fuer roloFlash, die noch eine aeltere Firmware als v07.** haben, wird
einmalig ein Update des Bootloaders benoetigt. Dieser ist eine
Voraussetzung, um auf eine hoehere Version der Firmware zu gelangen.
Auch mit dem neuen Bootloader koennen Sie weiterhin auf aeltere Firware-
Versionen zurueckkehren.

Bitte beachten Sie genau die Anleitung zum Update des Bootloaders im
Handbuch unter "Aktualisieren des Bootloaders". Die Dateien
RF2A06ZZ.HMP und RF2_06ZZ.HMP kommen dafuer zum Einsatz.

